Assumptions

The motor losses do not affect the PE side. heat sink cools only the PE. Motor is cooled via the case. The thermal models are decoupled.

PWM strategy is sinusoidal PWM

Ease of manufacturing

THD den bahsedecek miyiz?

Cogging torque ve torque ripple’dan nasıl bahsedelim??